{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Planilha2","Centro"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Planilha2","index":0,"n_rows":1,"n_cols":1,"rows_kept":1,"cut":false,"hidden":false,"merged":[]}
["dfd"]

{"sheet":"Centro","index":1,"n_rows":5,"n_cols":16,"rows_kept":5,"cut":false,"hidden":false,"merged":[[0,0,0,3],[0,4,0,15],[1,0,1,3]]}
[null,null,null,null," CENTRO"]
["Total:",null,null,null,6110.64,0,null,null,0,6110.64,0,null,6110.64,"",null,77862.76920000001]
["Grupo","Código do material","Descrição do material","UN","Saldo contábil (Qt)","Contagem 1","Contagem 2","Contagem 3","Contagem final","Diferença (Qt)","Ajustes do saldo contábil (+/-)","Justificativa","Qt. Ajuste efetivo","Dif. (%)","Custo Unitário","Valor do ajuste"]
["ZFMA",702371,"COMB OLEO DIESEL ","L",5355,{"$f":"'[1]Cálculo Diesel - Tanque 1'!B12+'[1]Cálculo Diesel - Tanque 2'!B12+'[1]Diesel Tambores'!A8","v":{"$error":"#VALUE!"}},null,null,0,5355,null,null,5355,1,3.6,19278]
["ZBIO",706515,"LENHA DE EUCALIPTO","ST",755.64,{"$f":"'[1]Lanç. Medições Lenha 706515'!L43","v":"TOTAL "},0,null,0,755.64,null,null,755.64,1,77.53,58584.769200000002]